;****************************************************************************************
;
;   mtkwl6ex.inf
;   MediaTek Wireless LAN card installation script
;
;   MediaTek Inc. (C)2024. All rights reserved.
;
;****************************************************************************************

[Version]
Signature       = "$Windows NT$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %MediaTek%
CatalogFile     = mtkwl6ex.cat
DriverVer       = 12/25/2024, 3.04.00.1159
PnpLockDown     = 1
[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%MediaTek%        = MediaTek, NTAMD64.10.0...16299

;*******************************************************************************************
; Win10 specific entries
;*******************************************************************************************
[MediaTek.NTAMD64.10.0...16299]
; MT7921 / MT7921K
%Generic.DeviceDescEx%          = MTK7921_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7961&SUBSYS_796114C3
%MT7921.DeviceDescExA%          = MTK7921_MODE3.ndi,      PCI\VEN_14C3&DEV_7961&SUBSYS_46801A3B
%MT7921.DeviceDescExA%          = MTK7921_MODE3.ndi,      PCI\VEN_14C3&DEV_7961&SUBSYS_46831A3B
%MT7921.DeviceDescExA%          = MTK7921_MODE1.ndi,      PCI\VEN_14C3&DEV_7961&SUBSYS_380211AD
%MT7921.DeviceDescExA%          = MTK7921_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7961&SUBSYS_46811A3B
%MT7921.DeviceDescExA%          = MTK7921_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7961&SUBSYS_46841A3B
%RZ608.DeviceDescExA%           = AMD7921_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0608&SUBSYS_060814C3
%RZ608.DeviceDescExA%           = AMD7921_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0608&SUBSYS_C60814C3
%RZ608.DeviceDescExA%           = AMD7921_MODE4.ndi,      PCI\VEN_14C3&DEV_0608&SUBSYS_E0D0105B
%RZ608.DeviceDescExA%           = AMD7921_MODE2.ndi,      PCI\VEN_14C3&DEV_0608&SUBSYS_E0C517AA
%MT7921.DeviceDescExA%          = MTK7921_MODE7.ndi,      PCI\VEN_14C3&DEV_7961&SUBSYS_E0B7105B
%MT7921.DeviceDescExA%          = MTK7921_MODE4.ndi,      PCI\VEN_14C3&DEV_7961&SUBSYS_E0BC17AA
%MT7921.DeviceDescExA%          = MTK7921_MODE5.ndi,      PCI\VEN_14C3&DEV_7961&SUBSYS_381217AA
%MT7921.DeviceDescExC%          = MTK7921_MODE1.ndi,      PCI\VEN_14C3&DEV_7961&SUBSYS_46821A3B
%MT7921.DeviceDescExA%          = MTK7921_MODE1.ndi,      PCI\VEN_14C3&DEV_7961&SUBSYS_46851A3B

; MT7922
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_792214C3
%MT7922.DeviceDescExA%          = MTK7922_MODE8.ndi,      PCI\VEN_14C3&DEV_7922&SUBSYS_53001A3B
%MT7922.DeviceDescExA%          = MTK7922_MODE8.ndi,      PCI\VEN_14C3&DEV_7922&SUBSYS_59101A3B
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_59111A3B
%MT7922.DeviceDescExA%          = MTK7922_MODE8.ndi,      PCI\VEN_14C3&DEV_7922&SUBSYS_51401A3B
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_53011A3B
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_380411AD
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_38E411AD
%MT7922.DeviceDescExA%          = MTK7922_MODE9.ndi,      PCI\VEN_14C3&DEV_7922&SUBSYS_E0DA105B
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_51411A3B
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_59141A3B
%RZ616.DeviceDescExA%           = AMD7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0616&SUBSYS_061614C3
%RZ616.DeviceDescExA%           = AMD7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0616&SUBSYS_C61614C3
%RZ616.DeviceDescExA%           = AMD7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0616&SUBSYS_D61614C3
%RZ616.DeviceDescExA%           = AMD7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0616&SUBSYS_E61614C3
%RZ616.DeviceDescExA%           = AMD7922_MODE1.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_E0C617AA
%RZ616.DeviceDescExA%           = AMD7922_MODE1.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_E0C717AA
%RZ616.DeviceDescExC%           = AMD7922_MODE5.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_E0CB105B
%RZ616.DeviceDescExC%           = AMD7922_MODE7.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_E0DB105B
%RZ616.DeviceDescExD%           = AMD7922_MODE6.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_E0CD105B
%RZ616.DeviceDescExD%           = AMD7922_MODE6.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_E0DE105B
%RZ616.DeviceDescExD%           = AMD7922_MODE6.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_E0DF105B
%RZ616.DeviceDescExD%           = AMD7922_MODE6.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_59171A3B
%RZ616.DeviceDescExD%           = AMD7922_MODE6.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_51421A3B
%RZ616.DeviceDescExA%           = AMD7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0616&SUBSYS_E0CF105B
%RZ616.DeviceDescExA%           = AMD7922_MODE3.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_E0D1105B
%RZ616.DeviceDescExA%           = AMD7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0616&SUBSYS_E0EC105B
%RZ616.DeviceDescExC%           = AMD7922_MODE7.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_223C14C3
%RZ616.DeviceDescExC%           = AMD7922_MODE7.ndi,      PCI\VEN_14C3&DEV_0616&SUBSYS_E0F8105B
%RZ616.DeviceDescExA%           = AMD7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0616&SUBSYS_E10B105B
%RZ616.DeviceDescExA%           = AMD7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_0616&SUBSYS_59151A3B
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_E132105B
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_E13B105B
%MT7922.DeviceDescExA%          = MTK7922_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7922&SUBSYS_E13C105B

; MT7920
%MT7920.DeviceDescExA%          = MTK7920_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7920&SUBSYS_792014C3
%MT7920.DeviceDescExA%          = MTK7920_MODE2.ndi,      PCI\VEN_14C3&DEV_7920&SUBSYS_E02017AA
%MT7920.DeviceDescExA%          = MTK7920_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7920&SUBSYS_64701A3B
%MT7920.DeviceDescExA%          = MTK7920_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7920&SUBSYS_64711A3B
%MT7920.DeviceDescExA%          = MTK7920_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7920&SUBSYS_64721A3B
%MT7920.DeviceDescExA%          = MTK7920_MODE1.ndi,      PCI\VEN_14C3&DEV_7920&SUBSYS_E120105B
%MT7920.DeviceDescExA%          = MTK7920_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7920&SUBSYS_8DD3103C
%MT7920.DeviceDescExA%          = MTK7920_DEFAULT.ndi,    PCI\VEN_14C3&DEV_7920&SUBSYS_380711AD

; MT7902
%MT7902.DeviceDescExA%          = MTK7902_MODE11.ndi,     PCI\VEN_14C3&DEV_7902&SUBSYS_790214C3
%MT7902.DeviceDescExA%          = MTK7902_MODE11.ndi,     PCI\VEN_14C3&DEV_7902&SUBSYS_0902185F
%MT7902.DeviceDescExA%          = MTK7902_MODE8.ndi,      PCI\VEN_14C3&DEV_7902&SUBSYS_55201A3B
%MT7902.DeviceDescExA%          = MTK7902_MODE11.ndi,     PCI\VEN_14C3&DEV_7902&SUBSYS_55211A3B
%MT7902.DeviceDescExB%          = MTK7902_MODE11.ndi,     PCI\VEN_14C3&DEV_7902&SUBSYS_55241A3B
%MT7902.DeviceDescExA%          = MTK7902_MODE10.ndi,     PCI\VEN_14C3&DEV_7902&SUBSYS_1EDE14C3
%MT7902.DeviceDescExB%          = MTK7902_MODE11.ndi,     PCI\VEN_14C3&DEV_7902&SUBSYS_380611AD
%MT7902.DeviceDescExC%          = MTK7902_MODE8.ndi,      PCI\VEN_14C3&DEV_7902&SUBSYS_60401A3B
%MT7902.DeviceDescExC%          = MTK7902_MODE11.ndi,     PCI\VEN_14C3&DEV_7902&SUBSYS_60411A3B
%MT7902.DeviceDescExA%          = MTK7902_MODE8.ndi,      PCI\VEN_14C3&DEV_7902&SUBSYS_004117F9
%MT7902.DeviceDescExA%          = MTK7902_MODE11.ndi,     PCI\VEN_14C3&DEV_7902&SUBSYS_E0DD105B
%MT7902.DeviceDescExA%          = MTK7902_MODE11.ndi,     PCI\VEN_14C3&DEV_7902&SUBSYS_E13F105B

;*******************************************************************************************
; MediaTek MT7920 default configuration
;*******************************************************************************************
[MTK7920_DEFAULT.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BandSelectionNo6G.reg,  MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, FWLogToHost.reg, RoamingAggreThMedLow.reg, Wifi6gCFG.reg, Coex.reg, BTDLPatch.reg, DeInitLP.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11
[MTK7920_DEFAULT.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog
[MTK7920_DEFAULT.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg
;*******************************************************************************************
; MediaTek MT7921 default configuration
;*******************************************************************************************
[MTK7921_DEFAULT.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, FWLogToHost.reg, Wifi6gCFG.reg, BandSelectionNo6G.reg, RoamingAggreThMedLow.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7921_DEFAULT.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7921_DEFAULT.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7922 default configuration
;*******************************************************************************************
[MTK7922_DEFAULT.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Wifi6gCFG.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11
[MTK7922_DEFAULT.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog
[MTK7922_DEFAULT.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7920 mode 1 configuration
;*******************************************************************************************
[MTK7920_MODE1.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BandSelectionNo6G.reg,  MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, FWLogToHost.reg, Wifi6gCFG.reg, RoamingAggreThMedLow.reg, Coex.reg, BTDLPatch.reg, EthernetDetectionMode1.reg, DmaRemappingEnable.reg, DeInitLP.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11
[MTK7920_MODE1.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog
[MTK7920_MODE1.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7920 mode 2 configuration
;*******************************************************************************************
[MTK7920_MODE2.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BandSelectionNo6G.reg,  MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, FWLogToHost.reg, Wifi6gCFG.reg, RoamingAggreThMedLow.reg, Coex.reg, BTDLPatch.reg, EthernetDetectionMode2.reg, DeInitLP.reg, EnergyStarEnable.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11
[MTK7920_MODE2.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog
[MTK7920_MODE2.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7921 mode 1 configuration
;*******************************************************************************************
[MTK7921_MODE1.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegionM1.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, Coex.reg, FWLogToHost.reg, Wifi6gCFG.reg, BandSelectionNo6G.reg, RoamingAggreThMedLow.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7921_MODE1.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7921_MODE1.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek mode 2 configuration
;*******************************************************************************************
[MTKWLAN_MODE2.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegionM1.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBandNoPref.reg, Wpp.reg, FWLogToHost.reg, EthernetDetectionMode2.reg, RoamingAggreThMedLow.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTKWLAN_MODE2.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTKWLAN_MODE2.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7921 mode 3 configuration
;     PreferredBand = 5G
;*******************************************************************************************
[MTK7921_MODE3.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegionM1.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBand5G.reg, Wpp.reg, FWLogToHost.reg, DeInitLP.reg, Wifi6gCFG.reg, BandSelectionNo6G.reg, RoamingAggreThMedLow.reg, SrrcDoubleSku.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7921_MODE3.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7921_MODE3.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7921 mode 4 configuration
;*******************************************************************************************
[MTK7921_MODE4.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegionM1.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, Coex.reg, FWLogToHost.reg, EthernetDetectionMode2.reg, BandSelectionNo6G.reg, RoamingAggreThMedLow.reg, SrrcDoubleSku.reg, EnergyStarEnable.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7921_MODE4.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7921_MODE4.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7921 mode 5 configuration
;*******************************************************************************************
[MTK7921_MODE5.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegionM1.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, Coex.reg, FWLogToHost.reg, EthernetDetectionMode2.reg, BandSelectionNo6G.reg, RoamingAggreThMedLow.reg, EnergyStarEnable.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7921_MODE5.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7921_MODE5.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7922 mode 6 configuration
;*******************************************************************************************
[MTK7922_MODE6.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, HotspotMCCEnable.reg, Wifi6gCFG.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7922_MODE6.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7922_MODE6.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7921 mode 7 configuration
;*******************************************************************************************
[MTK7921_MODE7.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegionM1.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, FWLogToHost.reg, EthernetDetectionMode1.reg, Coex.reg, BandSelectionNo6G.reg, RoamingAggreThMedLow.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7921_MODE7.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7921_MODE7.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7922 mode 8 configuration
;*******************************************************************************************
[MTK7922_MODE8.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, HotspotMCCEnable.reg, DeInitLP.reg, Wifi6gCFG.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, SrrcDoubleSku.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7922_MODE8.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7922_MODE8.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7902 mode 8 configuration
;*******************************************************************************************
[MTK7902_MODE8.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, HotspotMCCEnable.reg, DeInitLP.reg, Wifi6gCFG.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, SrrcDoubleSku.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11
[MTK7902_MODE8.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog
[MTK7902_MODE8.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg
;*******************************************************************************************
; MediaTek MT7922 mode 9 configuration
;*******************************************************************************************
[MTK7922_MODE9.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegionM1.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBandNoPref.reg, Wpp.reg, FWLogToHost.reg, EthernetDetectionMode1.reg, Enhance6G.reg, Coex.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, DmaRemappingEnable.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7922_MODE9.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7922_MODE9.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; MediaTek MT7902 mode 10 configuration
;*******************************************************************************************
[MTK7902_MODE10.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11
[MTK7902_MODE10.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog
[MTK7902_MODE10.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg
;*******************************************************************************************
; MediaTek MT7902 mode 11 configuration
;*******************************************************************************************
[MTK7902_MODE11.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Wifi6gCFG.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[MTK7902_MODE11.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[MTK7902_MODE11.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************

;*******************************************************************************************
; AMD 7922 default configuration
;*******************************************************************************************
[AMD7922_DEFAULT.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Wifi6gCFG.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11
[AMD7922_DEFAULT.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog
[AMD7922_DEFAULT.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg
;*******************************************************************************************
; AMD 7921 default configuration
;*******************************************************************************************
[AMD7921_DEFAULT.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, LedCust1.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, FWLogToHost.reg, Wifi6gCFG.reg, BandSelectionNo6G.reg, RoamingAggreThMedLow.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[AMD7921_DEFAULT.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7921_DEFAULT.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; AMD 7922 mode 1 configuration
;*******************************************************************************************
[AMD7922_MODE1.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, EthernetDetectionMode2.reg, Coex.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, SrrcDoubleSku.reg, AFC.reg, EnergyStarEnable.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[AMD7922_MODE1.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7922_MODE1.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; AMD 7921 mode 2 configuration
;*******************************************************************************************
[AMD7921_MODE2.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, FWLogToHost.reg, EthernetDetectionMode2.reg, BandSelectionNo6G.reg, RoamingAggreThMedLow.reg, EnergyStarEnable.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[AMD7921_MODE2.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7921_MODE2.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; AMD 7922 mode 3 configuration
;*******************************************************************************************
[AMD7922_MODE3.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, HotspotMCCEnable.reg, Wifi6gCFG.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[AMD7922_MODE3.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7922_MODE3.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; AMD 7921 mode 4 configuration
;*******************************************************************************************
[AMD7921_MODE4.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegionM2.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNo6G.reg, Wpp.reg, FWLogToHost.reg, HotspotMCCTputOptimization.reg, BandSelectionNo6G.reg, RoamingAggreThMedLow.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[AMD7921_MODE4.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7921_MODE4.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; AMD 7922 mode 5 configuration
;*******************************************************************************************
[AMD7922_MODE5.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[AMD7922_MODE5.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7922_MODE5.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; AMD 7922 mode 6 configuration
;*******************************************************************************************
[AMD7922_MODE6.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, HotspotMCCEnable.reg, DeInitLP.reg, Wifi6gCFG.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, SrrcDoubleSku.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[AMD7922_MODE6.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7922_MODE6.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; AMD 7922 mode 7 configuration
;*******************************************************************************************
[AMD7922_MODE7.ndi.NT]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.CopyFiles
AddReg                  = Common.reg, BWSelection6G.reg, MTPCI_OS61.ndi.NT.reg, IHV.reg, CountryRegion.reg, IEEE80211H.reg, PsControl.reg, ChannelMode.reg, ThermalProtection.reg, Wow.reg, PreferBandNoPref.reg,Wpp.reg, FWLogToHost.reg, Enhance6G.reg, BandSelection6G.reg, RoamingAggreThMedLow.reg, AFC.reg
DelReg                  = RegRemove.delReg
Characteristics         = 0x84 ;NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType                 = 5 ;PCI
CopyFiles               = NT.CopyFiles, IHV.CopyFiles
*IfType                 = 71 ;IF_TYPE_IEEE80211
*MediaType              = 16 ;NdisMediumNative802_11
*PhysicalMediaType      = 9 ;NdisPhysicalMediumNative802_11

[AMD7922_MODE7.ndi.NT.Services]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.Services
AddService              = %ServiceName%,2,Generic.Service,common.EventLog

[AMD7922_MODE7.ndi.NT.HW]
Include                 = netvwifibus.inf
Needs                   = VWiFiBus.PnPFilterRegistration.Hw
AddReg                  = MSI.reg

;*******************************************************************************************
; Regs for NT
;*******************************************************************************************
[Common.reg]
HKR,,CCXPktLossLimitTime,0,"30"
HKR,,CCXDbmOffset,0,"4"
HKR,,CACDropPeriod,0,"0"
HKR,,CACDropCriteria,0,"1700"
HKR,,ConnIdleTimeForL1,0,"0"
HKR,,LowPowerEnable,0,"1"
HKR,,WirelessMode,0,"11"
HKR,,TXBurst,0,"1"
HKR,,BinMode,0,"0"
HKR,,DowngradeTxStreamFeatureEnable,0,"1"
HKR,,DowngradeTxStreamLowTempEnable,0,"1"
HKR,,DowngradeTxStreamLowTemp,0,"110"
HKR,,DowngradeTxStreamHighTempEnable,0,"1"
HKR,,DowngradeTxStreamHighTemp,0,"120"
HKR,,ShortSlot,0,"1"
HKR,,AdhocOfdm,0,"1"
HKR,,Adhoc5GDisable,0,"0"
HKR,,AdhocN40MHzAllowed,0,"0"
HKR,,WSCVersion2,0x00010001,0x00000020
HKR,,WSC20Testbed,0x00010001,0x0000000C
HKR,,MFPC,0,"1"
HKR,,InBoxMode,0,"0"
HKR,,Channel,0,%CHANNEL%
HKR,Default,Channel,0,%CHANNEL%
HKR,,RDG,0,"0"
HKR,,WMMCapable,0,"1"
HKR,,CarrierDetect,0,"0"
HKR,,MFPM3,0,"0"
HKR,,Radio,0x10001,0x7
HKR,,EnableSystemEventLog,0,"1"
HKR,,AbortTaskImprovement,0,"0"

;
; CurrPhyMode
;
HKR, ,                              CurrPhyMode,     0, "0"
HKR, NDI\params\CurrPhyMode,        ParamDesc,       0, %CurrPhyMode%
HKR, NDI\params\CurrPhyMode,        type,            0, "enum"
HKR, NDI\params\CurrPhyMode,        default,         0, "0"
HKR, NDI\params\CurrPhyMode\enum,   "0",             0, "1. "%Phy_11ax%
HKR, NDI\params\CurrPhyMode\enum,   "1",             0, "2. "%Phy_11ac%
HKR, NDI\params\CurrPhyMode\enum,   "2",             0, "3. "%Phy_11n%
HKR, NDI\params\CurrPhyMode\enum,   "3",             0, "4. "%Phy_11abg%
;
; BWSelection24G
;
HKR, ,                                 BWSelection24G,          0, "0"
HKR, NDI\params\BWSelection24G,        ParamDesc,               0, %BWSelection24G%
HKR, NDI\params\BWSelection24G,        type,                    0, "enum"
HKR, NDI\params\BWSelection24G,        default,                 0, "0"
HKR, NDI\params\BWSelection24G\enum,   "0",                     0, "1. "%BW_Auto%
HKR, NDI\params\BWSelection24G\enum,   "1",                     0, "2. "%BW_20%
;
; BWSelection5G
;
HKR, ,                                 BWSelection5G,           0, "0"
HKR, NDI\params\BWSelection5G,         ParamDesc,               0, %BWSelection5G%
HKR, NDI\params\BWSelection5G,         type,                    0, "enum"
HKR, NDI\params\BWSelection5G,         default,                 0, "0"
HKR, NDI\params\BWSelection5G\enum,    "0",                     0, "1. "%BW_Auto%
HKR, NDI\params\BWSelection5G\enum,    "1",                     0, "2. "%BW_20%
;
; DisableWakeOnMagic
;
HKR, NDI\params\DisableWakeOnMagic,        ParamDesc,           0, %DisableWakeOnMagic%
HKR, NDI\params\DisableWakeOnMagic,        type,                0, "enum"
HKR, NDI\params\DisableWakeOnMagic,        default,             0, "0"
HKR, NDI\params\DisableWakeOnMagic\enum,   "1",                 0, %Disable%
HKR, NDI\params\DisableWakeOnMagic\enum,   "0",                 0, %Enable%
;
; DisableWakeOnPattern
;
HKR, NDI\params\DisableWakeOnPattern,        ParamDesc,               0, %DisableWakeOnPattern%
HKR, NDI\params\DisableWakeOnPattern,        type,                    0, "enum"
HKR, NDI\params\DisableWakeOnPattern,        default,                 0, "0"
HKR, NDI\params\DisableWakeOnPattern\enum,   "1",                     0, %Disable%
HKR, NDI\params\DisableWakeOnPattern\enum,   "0",                     0, %Enable%
;
; DisableARPOffload
;
HKR, NDI\params\DisableARPOffload,        ParamDesc,               0, %DisableARPOffload%
HKR, NDI\params\DisableARPOffload,        type,                    0, "enum"
HKR, NDI\params\DisableARPOffload,        default,                 0, "0"
HKR, NDI\params\DisableARPOffload\enum,   "1",                     0, %Disable%
HKR, NDI\params\DisableARPOffload\enum,   "0",                     0, %Enable%
;
; DisableGTKRekey
;
HKR, NDI\params\DisableGTKRekey,        ParamDesc,               0, %DisableGTKRekey%
HKR, NDI\params\DisableGTKRekey,        type,                    0, "enum"
HKR, NDI\params\DisableGTKRekey,        default,                 0, "0"
HKR, NDI\params\DisableGTKRekey\enum,   "1",                     0, %Disable%
HKR, NDI\params\DisableGTKRekey\enum,   "0",                     0, %Enable%
;
; UAPSDSupport
;
HKR, ,                               UAPSDSupport,            0, "0"
HKR, NDI\params\UAPSDSupport,        ParamDesc,               0, %UAPSDSupport%
HKR, NDI\params\UAPSDSupport,        type,                    0, "enum"
HKR, NDI\params\UAPSDSupport,        default,                 0, "0"
HKR, NDI\params\UAPSDSupport\enum,   "1",                     0, %Enable%
HKR, NDI\params\UAPSDSupport\enum,   "0",                     0, %Disable%
;
; AMSDUTx
;
HKR, NDI\params\AMSDUTx,        ParamDesc,               0, %AMSDUTx%
HKR, NDI\params\AMSDUTx,        type,                    0, "enum"
HKR, NDI\params\AMSDUTx,        default,                 0, "1"
HKR, NDI\params\AMSDUTx\enum,   "1",                     0, %Enable%
HKR, NDI\params\AMSDUTx\enum,   "0",                     0, %Disable%
;
; AMSDURx
;
HKR, NDI\params\AMSDURx,        ParamDesc,               0, %AMSDURx%
HKR, NDI\params\AMSDURx,        type,                    0, "enum"
HKR, NDI\params\AMSDURx,        default,                 0, "1"
HKR, NDI\params\AMSDURx\enum,   "1",                     0, %Enable%
HKR, NDI\params\AMSDURx\enum,   "0",                     0, %Disable%

HKR,,BACapability,0x10001,"0x0b834040"
HKR,Default,BACapability,0x10001,"0x0b834040"
HKR,,WifiDirectControl,0x10001,"0x84368078"
HKR,Default,WifiDirectControl,0x10001,"0x84368078"
HKR,,WfdListenChannel,0,"11"
HKR,Default,WfdListenChannel,0,"11"
HKR,,WfdPhyMode,0,"1"
HKR,Default,WfdPhyMode,0,"1"
;
; Miracast prefer band
;
HKR,,WfdGOOperatingChannel,0,"0"
HKR,NDI\params\WfdGOOperatingChannel,ParamDesc,0, "Miracast prefer band"
HKR,NDI\params\WfdGOOperatingChannel,type,     0, "enum"
HKR,NDI\params\WfdGOOperatingChannel,default,  0, "0"
HKR,NDI\params\WfdGOOperatingChannel\enum,     0,0, %WirelessModeAuto%
HKR,NDI\params\WfdGOOperatingChannel\enum,     11,0, %WirelessMode24G%
HKR,NDI\params\WfdGOOperatingChannel\enum,     36,0, %WirelessMode5G%
HKR,,P2P_GO_Band,0,"2"
HKR,Default,P2P_GO_Band,0,"2"
HKR,,Enable_U4TVBOX_FIX,0,"1"
HKR,Default,Enable_U4TVBOX_FIX,0,"1"
HKR,,P2PAckCheck,0,"1"
HKR,Default,P2PAckCheck,0,"1"
HKR,,P2PVideoBoost,0,"0"
HKR,,TransmitSetting,0x10001,"0x22d8f9"
HKR,Default,TransmitSetting,0x10001,"0x22d8f9"
HKR,,WPSDevName,0,%WPS_DEVNAME_DEF_STR%
HKR,Default,WPSDevName,0,%WPS_DEVNAME_DEF_STR%
HKR,,ProhibitTKIPonHT,0,"1"
HKR,,LinkSpeedStatus,0,"0"
;
; Low power
;
HKR, NDI\params\LowPowerEnable,        ParamDesc,               0, %LowpowerStr%
HKR, NDI\params\LowPowerEnable,        type,                    0, "enum"
HKR, NDI\params\LowPowerEnable,        default,                 0, "1"
HKR, NDI\params\LowPowerEnable\enum,   "0",                     0, %Disable%
HKR, NDI\params\LowPowerEnable\enum,   "1",                     0, %WirelessModeAuto%
;
; TxPowerLevel
;
HKR, ,                                TxPowerLevel,           0, "0"
HKR, NDI\params\TxPowerLevel,         ParamDesc,              0, %TxPowerLevel%
HKR, NDI\params\TxPowerLevel,         type,                   0, "enum"
HKR, NDI\params\TxPowerLevel,         default,                0, "0"
HKR, NDI\params\TxPowerLevel\enum,    "0",                    0, "1. "%Highest%
HKR, NDI\params\TxPowerLevel\enum,    "1",                    0, "2. "%Medium%
HKR, NDI\params\TxPowerLevel\enum,    "2",                    0, "3. "%Lowest%

[BWSelection6G.reg]
;
; BWSelection6G
;
HKR, ,                                 BWSelection6G,           0, "0"
HKR, NDI\params\BWSelection6G,         ParamDesc,               0, %BWSelection6G%
HKR, NDI\params\BWSelection6G,         type,                    0, "enum"
HKR, NDI\params\BWSelection6G,         default,                 0, "0"
HKR, NDI\params\BWSelection6G\enum,    "0",                     0, "1. "%BW_Auto%
HKR, NDI\params\BWSelection6G\enum,    "1",                     0, "2. "%BW_20%
[Wpp.reg]
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, Start, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, BufferSize, 0x00010001, 0x50
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, ClockType, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, FileMax, 0x00010001, 0x4
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, FileName, 0, "%%SystemRoot%%\System32\LogFiles\WMI\MTK\mtkwl.etl"
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, Guid, 0, "{6E7426BF-2100-4E08-9925-0F77AC45DEA6}"
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, LogFileMode, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, MaxFileSize, 0x00010001, 0x32
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, MaximumBuffers, 0x00010001, 0x10
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL, MinimumBuffers, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL\{04E020C0-4996-4C83-AF91-A6484F61B360}, Enabled, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL\{04E020C0-4996-4C83-AF91-A6484F61B360}, EnableLevel, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWL\{04E020C0-4996-4C83-AF91-A6484F61B360}, EnableFlags, 0x00010001, 0x7fffffff

[FWLogToHost.reg]
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, Start, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, BufferSize, 0x00010001, 0x50
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, ClockType, 0x00010001, 0x1
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, FileMax, 0x00010001, 0x3
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, FileName, 0, "%%SystemRoot%%\System32\LogFiles\WMI\MTK\mtkwlFW.etl"
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, Guid, 0, "{6E7426BF-2100-4E08-9925-0F77AC45DEA6}"
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, LogFileMode, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, MaxFileSize, 0x00010001, 0xc8
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, MaximumBuffers, 0x00010001, 0x10
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, MinimumBuffers, 0x00010001, 0x2
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW, FWToHost, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW\{A6053918-A813-4451-9421-47845504CDAB}, Enabled, 0x00010001, 0x0
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW\{A6053918-A813-4451-9421-47845504CDAB}, EnableLevel, 0x00010001, 0x5
HKLM, SYSTEM\CurrentControlSet\Control\WMI\AutoLogger\MTKWLFW\{A6053918-A813-4451-9421-47845504CDAB}, EnableFlags, 0x00010001, 0x7fffffff

[IHV.reg]
HKR,Ndi\IHVExtensions,ExtensibilityDLL,0,"%%SystemRoot%%\system32\mtkihvx.dll"

[IEEE80211H.reg]
HKR,,IEEE80211H,0,"0"

[Coex.reg]
HKR,,CoexGModeRate,0,"1"
HKR,,EnDefaultIotApRule,0,"1"

[DynAdvSwitchV2.reg]
HKR,,DynAdvV2En,0,"1"

[PsControl.reg]
HKR,,PSMControl,0x00010001,0x00000000

[CountryRegion.reg]
HKR,,CountryRoamingEn,0,"1"
HKR,,SmartCountryDecisionEn,0,"0"
HKR,,DynamicCountryDecisionEn,0,"1"
HKR,,CountryRegionString,0,"WW"
HKR,,CountryDecisionNum,0,"1"
HKR,,CSSCode,0,"0"

[CountryRegionM1.reg]
HKR,,CountryRoamingEn,0,"1"
HKR,,SmartCountryDecisionEn,0,"0"
HKR,,DynamicCountryDecisionEn,0,"1"
HKR,,CountryRegionString,0,"WW"
HKR,,CountryDecisionNum,0,"1"
HKR,,CSSCode,0,"0"

[CountryRegionM2.reg]
HKR,,CountryRoamingEn,0,"1"
HKR,,SmartCountryDecisionEn,0,"0"
HKR,,DynamicCountryDecisionEn,0,"1"
HKR,,CountryRegionString,0,"WW"
HKR,,CountryDecisionNum,0,"1"
HKR,,CSSCode,0,"B"

[DisableCountryRoaming.reg]
HKR,,CountryRoamingEn,0,"0"
HKR,,SmartCountryDecisionEn,0,"1"
HKR,,DynamicCountryDecisionEn,0,"1"
HKR,,CountryRegionString,0,"WW"
HKR,,CountryDecisionNum,0,"1"

[LedCust1.reg]
HKR,,LedCustMode,0,"1"
HKR,,OemLedMode,0,"1"

[Wow.reg]
HKR,,WakeUpCapabilities,0x00010001,0x0005DFFF
HKR,,WakeUpFuncEnable,0x00010001,0x0007
HKR,,ETxBfNonCompressedFeedback,0,"0"

[MSI.reg]
HKR,Interrupt Management,,0x00000010
HKR,Interrupt Management\MessageSignaledInterruptProperties,,0x00000010
HKR,Interrupt Management\MessageSignaledInterruptProperties,MSISupported,0x00010001,1
HKR,Interrupt Management\MessageSignaledInterruptProperties,MessageNumberLimit,0x00010001,1

[ChannelMode.reg]
HKR,,ChannelMode,0,"1"

[ThermalProtection.reg]
HKR,,ThermalProtectHighEn,0,"1"
HKR,,ThermalProtectHigh,0,"88"
HKR,,ThermalProtectLowEn,0,"1"
HKR,,ThermalProtectLow,0,"80"

[EthernetDetectionMode1.reg]
HKR,,EthernetDetection,0,"2"
HKR,,EthernetDetectionInterval,0,"2000"

[EthernetDetectionMode2.reg]
HKR,,EthernetDetection,0,"1"
HKR,,EthernetDetectionInterval,0,"5000"

[HotspotMCCEnable.reg]
HKR,,HotspotMCCEnable,0,"0"

[HotspotMCCTputOptimization.reg]
HKR,,HotspotMCCTputOptimization,0,"1"

[PreferBandNoPref.reg]
;
; PreferredBand
;
HKR, NDI\params\PreferredBand,        ParamDesc,       0, %PreferredBand%
HKR, NDI\params\PreferredBand,        type,            0, "enum"
HKR, NDI\params\PreferredBand,        default,         0, "0"
HKR, NDI\params\PreferredBand\enum,   "0",             0, "1. "%NoPref%
HKR, NDI\params\PreferredBand\enum,   "1",             0, "2. "%Band_24G%
HKR, NDI\params\PreferredBand\enum,   "2",             0, "3. "%Band_5G%
HKR, NDI\params\PreferredBand\enum,   "3",             0, "4. "%Band_6G%

[PreferBand5G.reg]
;
; PreferredBand
;
HKR, NDI\params\PreferredBand,        ParamDesc,       0, %PreferredBand%
HKR, NDI\params\PreferredBand,        type,            0, "enum"
HKR, NDI\params\PreferredBand,        default,         0, "2"
HKR, NDI\params\PreferredBand\enum,   "0",             0, "1. "%NoPref%
HKR, NDI\params\PreferredBand\enum,   "1",             0, "2. "%Band_24G%
HKR, NDI\params\PreferredBand\enum,   "2",             0, "3. "%Band_5G%

[PreferBandNo6G.reg]
;
; PreferredBand
;
HKR, NDI\params\PreferredBand,        ParamDesc,       0, %PreferredBand%
HKR, NDI\params\PreferredBand,        type,            0, "enum"
HKR, NDI\params\PreferredBand,        default,         0, "0"
HKR, NDI\params\PreferredBand\enum,   "0",             0, "1. "%NoPref%
HKR, NDI\params\PreferredBand\enum,   "1",             0, "2. "%Band_24G%
HKR, NDI\params\PreferredBand\enum,   "2",             0, "3. "%Band_5G%

[BandSelection6G.reg]
;
; BandSelection
;
HKR, ,                                 BandSelection,          0, "0" 
HKR, NDI\params\BandSelection,         ParamDesc,              0, %BandSelection%
HKR, NDI\params\BandSelection,         type,                   0, "enum"
HKR, NDI\params\BandSelection,         default,                0, "0"
HKR, NDI\params\BandSelection\enum,    "0",                    0, "1. "%Band_All%
HKR, NDI\params\BandSelection\enum,    "1",                    0, "2. "%Band24G%
HKR, NDI\params\BandSelection\enum,    "2",                    0, "3. "%Band5G%
HKR, NDI\params\BandSelection\enum,    "3",                    0, "4. "%Band6G%

[BandSelectionNo6G.reg]
;
; BandSelection
;
HKR, ,                                 BandSelection,          0, "0" 
HKR, NDI\params\BandSelection,         ParamDesc,              0, %BandSelection%
HKR, NDI\params\BandSelection,         type,                   0, "enum"
HKR, NDI\params\BandSelection,         default,                0, "0"
HKR, NDI\params\BandSelection\enum,    "0",                    0, "1. "%Band_All%
HKR, NDI\params\BandSelection\enum,    "1",                    0, "2. "%Band24G%
HKR, NDI\params\BandSelection\enum,    "2",                    0, "3. "%Band5G%

[RoamingAggreThMedLow.reg]
;
; Roaming Aggressiveness
;
HKR,,RoamIndicateTh,0,"2"
HKR, NDI\params\RoamIndicateTh, ParamDesc, 0, %RoamingAggressiveness%
HKR, NDI\params\RoamIndicateTh, type, 0, "enum"
HKR, NDI\params\RoamIndicateTh, default, 0, "3"
HKR, NDI\params\RoamIndicateTh\enum, "0", 0, "1. "%Disable%
HKR, NDI\params\RoamIndicateTh\enum, "1", 0, "2. "%Lowest%
HKR, NDI\params\RoamIndicateTh\enum, "2", 0, "3. "%MediumLow%
HKR, NDI\params\RoamIndicateTh\enum, "3", 0, "4. "%Medium%
HKR, NDI\params\RoamIndicateTh\enum, "4", 0, "5. "%MediumHigh%
HKR, NDI\params\RoamIndicateTh\enum, "5", 0, "6. "%Highest%

[DeInitLP.reg]
HKR,,DeInitLP,0,"1"

[Enhance6G.reg]
HKR,,Enable6GEnhance,0,"1"

[RegRemove.delReg]
HKR,,CurrPhyMode
HKR, NDI\params\CurrPhyMode
HKR,,RoamIndicateTh
HKR, NDI\params\RoamIndicateTh
HKR,,BandSelection
HKR, NDI\params\BandSelection
HKR,,LowPowerEnable
HKR, NDI\params\LowPowerEnable

[Wifi6gCFG.reg]
HKR,,Win10dis6G,0,"0"

[SrrcDoubleSku.reg]
HKR,,ForceSRRCNewRulePwr,0,"0"

[BTDLPatch.reg]
HKR,,LoadBtPatchEn,0,"1"

[AFC.reg]
HKR,,AFCEnable,0,"1"
HKR,,AfcBackoffPwrLimit,0,"0"

[DmaRemappingEnable.reg]
HKR,,DmaRemappingEn,0,"1"

[EnergyStarEnable.reg]
HKR,,EnergyStarEnable ,0,"1"

;*******************************************************************************************
; DestinationDirs
;*******************************************************************************************
[NT.CopyFiles]
mtkwl6ex.sys,,,2
;mtkwlan.dat,,,2
WIFI_MT7961_patch_mcu_1a_2_hdr.bin,,,2
WIFI_RAM_CODE_MT7961_1a.bin,,,2
WIFI_MT7961_patch_mcu_1_2_hdr.bin,,,2
WIFI_RAM_CODE_MT7961_1.bin,,,2
WIFI_MT7922_patch_mcu_1_1_hdr.bin,,,2
WIFI_RAM_CODE_MT7922_1.bin,,,2
WIFI_MT7902_patch_mcu_1_1_hdr.bin,,,2
WIFI_RAM_CODE_MT7902_1.bin,,,2
mtkwl1.dat,,,2
mtkwl2.dat,,,2
mtkwl2s.dat,,,2
mtkwl3.dat,,,2
mtkwl1_2.dat,,,2
mtkwl2_2.dat,,,2
mtkwl2_2s.dat,,,2
mtkwl3_2.dat,,,2
mtkwl4.dat,,,2

[IHV.CopyFiles]
mtkihvx.dll,,,2

[SourceDisksNames]
1 = %INSTALL_DISK_STR%,,,

[SourceDisksFiles]
mtkwl6ex.sys                          = 1,,
mtkihvx.dll                           = 1,,
;mtkwlan.dat                           = 1,,
WIFI_MT7961_patch_mcu_1a_2_hdr.bin    = 1,,
WIFI_RAM_CODE_MT7961_1a.bin           = 1,,
WIFI_MT7961_patch_mcu_1_2_hdr.bin     = 1,,
WIFI_RAM_CODE_MT7961_1.bin            = 1,,
WIFI_MT7922_patch_mcu_1_1_hdr.bin     = 1,,
WIFI_RAM_CODE_MT7922_1.bin            = 1,,
WIFI_MT7902_patch_mcu_1_1_hdr.bin     = 1,,
WIFI_RAM_CODE_MT7902_1.bin            = 1,,
mtkwl1.dat                            = 1,,
mtkwl2.dat                            = 1,,
mtkwl2s.dat                            = 1,,
mtkwl3.dat                            = 1,,
mtkwl1_2.dat                          = 1,,
mtkwl2_2.dat                            = 1,,
mtkwl2_2s.dat                            = 1,,
mtkwl3_2.dat                            = 1,,
mtkwl4.dat                            = 1,,

[DestinationDirs]
NT.CopyFiles            = 13 ; system32\drivers subdirectory on NT
DefaultDestDir          = 11
CoInstaller.CopyFiles   = 11
IHV.CopyFiles           = 11 ; Windows\System32

;*******************************************************************************************
; NT specific
;*******************************************************************************************
[MTPCI_OS61.ndi.NT.reg]
HKR,Ndi,Service,0,%ServiceName%
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,Ndi\Interfaces,LowerRange,0,"wlan,ethernet,vwifi"

[Generic.Service]
DisplayName            = %Generic.Service.DispName%
ServiceType            = 1 ;%SERVICE_KERNEL_DRIVER%
StartType              = 3 ;%SERVICE_AUTO_START%
ErrorControl           = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary          = %13%\mtkwl6ex.sys
LoadOrderGroup         = NDIS

[common.EventLog]
AddReg      = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR,,EventMessageFile,0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%13%%\mtkwl6ex.sys"
HKR,,TypesSupported,0x00010001,7

;*******************************************************************************************
; Strings
;*******************************************************************************************
[strings]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "Radio On/Off"
CountryRegion24G            = "Country Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Country Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Gaming Environment"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Preferred Band"
NoPref                      = "No Preference"
Band_24G                    = "Prefer 2.4GHz band"
Band_5G                     = "Prefer 5GHz band"
Band_6G                     = "Prefer 6GHz band"
DisableWakeOnMagic          = "Wake on Magic Packet"
DisableWakeOnPattern        = "Wake on Pattern Match"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Disabled"
Enable                      = "Enabled"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Roaming Aggressiveness" 
Lowest                      = "Lowest"
MediumLow                   = "Medium-Low"
Medium                      = "Medium"
MediumHigh                  = "Medium-High"
Highest                     = "Highest"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Traditional Chinese 
;*******************************************************************************************
[Strings.0404]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "無線裝置 開/關"
CountryRegion24G            = "頻道代碼 (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "頻道代碼 (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "多媒體/遊戲環境"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "偏好的頻帶"
NoPref                      = "無偏好設定"
Band_24G                    = "喜好 2.4 GHz 頻帶"
Band_5G                     = "偏好 5GHz 頻帶"
Band_6G                     = "偏好 6GHz 頻帶"
DisableWakeOnMagic          = "收到 Magic 封包時喚醒"
DisableWakeOnPattern        = "收到模式對應時喚醒"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "禁用"
Enable                      = "啟用"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "漫遊積極度" 
Lowest                      = "最低"
MediumLow                   = "中低"
Medium                      = "中"
MediumHigh                  = "中高"
Highest                     = "最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Simplified Chinese
;*******************************************************************************************
[Strings.0804]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "无线装置 开/关"
CountryRegion24G            = "频道代码 (2.4GHz)"
CountryRegion24G_0          = "#0 (1-11)"
CountryRegion24G_1          = "#1 (1-13)"
CountryRegion24G_2          = "#2 (10-11)"
CountryRegion24G_3          = "#3 (10-13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1-14)"
CountryRegion24G_6          = "#6 (3-9)"
CountryRegion24G_7          = "#7 (5-13)"
CountryRegion5G             = "频道代码(5GHz)"
CountryRegion5G_0           = "#0 (36-64,149-165)"
CountryRegion5G_1           = "#1 (36-140)"
CountryRegion5G_2           = "#2 (36-64)"
CountryRegion5G_3           = "#3 (52-64,149-161)"
CountryRegion5G_4           = "#4 (149-165)"
CountryRegion5G_5           = "#5 (149-161)"
CountryRegion5G_6           = "#6 (36-48)"
CountryRegion5G_7           = "#7 (36-165)"
CountryRegion5G_8           = "#8 (52-64)"
CountryRegion5G_9           = "#9 (36-116,132-165)"
CountryRegion5G_10          = "#10 (36-48,149-165)"
CountryRegion5G_11          = "#11 (36-120,149-161)"
CountryRegion5G_12          = "#12 (36-140)"
CountryRegion5G_13          = "#13 (52-161)"
CountryRegion5G_14          = "#14 (36-116,136-165)"
CountryRegion5G_15          = "#15 (149-173)"
CountryRegion5G_16          = "#16 (36-173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "多媒体/游戏环境"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "首选频带"
NoPref                      = "无首选项"
Band_24G                    = "首选 2.4 GHz 频带"
Band_5G                     = "首选 5GHz 频带"
Band_6G                     = "首选 6GHz 频带"
DisableWakeOnMagic          = "唤醒幻数据包"
DisableWakeOnPattern        = "唤醒模式匹配"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "已禁用"
Enable                      = "已启用"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "漫游主动性" 
Lowest                      = "最低"
MediumLow                   = "中低"
Medium                      = "中"
MediumHigh                  = "中高"
Highest                     = "最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "省电"

;*******************************************************************************************
; Strings --- Japanese
;*******************************************************************************************
[Strings.0411]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "無線デバイス オン/オフ"
CountryRegion24G            = "チャンネルコード  (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "チャンネルコード (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "マルチメディア/ゲーミング環境"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "優先バンド"
NoPref                      = "優先順位なし"
Band_24G                    = "2.4 GHz バンドの優先"
Band_5G                     = "5 GHz バンドを優先"
Band_6G                     = "6 GHz バンドを優先"
DisableWakeOnMagic          = "Wake on Magic Packet"
DisableWakeOnPattern        = "Wake on Pattern Match"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "無効"
Enable                      = "無効"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "ローミングの積極性" 
Lowest                      = "最低"
MediumLow                   = "中低"
Medium                      = "中"
MediumHigh                  = "中高"
Highest                     = "最高"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Korean
;*******************************************************************************************
[Strings.0412]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "라디오 ON/OFF"
CountryRegion24G            = "국가/지역  (2.4GHz)"
CountryRegion24G_0          = "#0 (1-11)"
CountryRegion24G_1          = "#1 (1-13)"
CountryRegion24G_2          = "#2 (10-11)"
CountryRegion24G_3          = "#3 (10-13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1-14)"
CountryRegion24G_6          = "#6 (3-9)"
CountryRegion24G_7          = "#7 (5-13)"
CountryRegion5G             = "국가/지역 (5GHz)"
CountryRegion5G_0           = "#0 (36-64,149-165)"
CountryRegion5G_1           = "#1 (36-140)"
CountryRegion5G_2           = "#2 (36-64)"
CountryRegion5G_3           = "#3 (52-64,149-161)"
CountryRegion5G_4           = "#4 (149-165)"
CountryRegion5G_5           = "#5 (149-161)"
CountryRegion5G_6           = "#6 (36-48)"
CountryRegion5G_7           = "#7 (36-165)"
CountryRegion5G_8           = "#8 (52-64)"
CountryRegion5G_9           = "#9 (36-116,132-165)"
CountryRegion5G_10          = "#10 (36-48,149-165)"
CountryRegion5G_11          = "#11 (36-120,149-161)"
CountryRegion5G_12          = "#12 (36-140)"
CountryRegion5G_13          = "#13 (52-161)"
CountryRegion5G_14          = "#14 (36-116,136-165)"
CountryRegion5G_15          = "#15 (149-173)"
CountryRegion5G_16          = "#16 (36-173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "멀티미디어/게임 환경"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "기본 설정 밴드"
NoPref                      = "기본 설정 없음"
Band_24G                    = "2.4 GHz 밴드 선택"
Band_5G                     = "5GHz 밴드 기본 설정"
Band_6G                     = "6GHz 밴드 기본 설정"
DisableWakeOnMagic          = "Wake on 매직 패킷"
DisableWakeOnPattern        = "Wake on 패턴 일치"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "비활성화함"
Enable                      = "활성화함"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "로밍의 주동성" 
Lowest                      = "최하"
MediumLow                   = "보통-낮음"
Medium                      = "보통"
MediumHigh                  = "보통-높음"
Highest                     = "최고"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- French
;*******************************************************************************************
[Strings.040c]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "Radio Marche/Arrêt"
CountryRegion24G            = "Pays / Région (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Pays / Région (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Environnements Multimédia/Jeux"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Bande privilégiée"
NoPref                      = "Aucune préférence"
Band_24G                    = "Préférer bande 2,4 GHz"
Band_5G                     = "Préférer la bande 5 GHz"
Band_6G                     = "Préférer la bande 6 GHz"
DisableWakeOnMagic          = "Wake on Magic Packet"
DisableWakeOnPattern        = "Correspondance au modèle WOL"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Désactivé(e)"
Enable                      = "Activé(e"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Agressivité de l’itinérance" 
Lowest                      = "Min."
MediumLow                   = "Faible"
Medium                      = "Moyenne"
MediumHigh                  = "Élevée"
Highest                     = "Max."

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Italian
;*******************************************************************************************
[Strings.0410]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "Radio Acceso/Spento"
CountryRegion24G            = "Paese (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Paese (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Ambiente multimediale/giochi"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Banda preferita"
NoPref                      = "Nessuna preferenza"
Band_24G                    = "Preferenza a banda a 2,4 GHz"
Band_5G                     = "Banda a 5 GHz"
Band_6G                     = "Banda a 6 GHz"
DisableWakeOnMagic          = "Magic Packet per riattivazione"
DisableWakeOnPattern        = "Corrispondenza motivo per riattivazione"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Disattivata"
Enable                      = "Attivata"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Efficacia roaming" 
Lowest                      = "Minimo"
MediumLow                   = "Medio-basso"
Medium                      = "Medio"
MediumHigh                  = "Medio-alto"
Highest                     = "Massimo"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- German
;*******************************************************************************************
[Strings.0407]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "Radio An/Aus"
CountryRegion24G            = "Land Region (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Land Region (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Spielumgebung"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Bevorzugtes Band"
NoPref                      = "Keine Einstellung"
Band_24G                    = "2,4-GHz-Band bevorzugen"
Band_5G                     = "5 GHz-Band bevorzugt"
Band_6G                     = "6 GHz-Band bevorzugt"
DisableWakeOnMagic          = "Aktivierung durch Magic Packet"
DisableWakeOnPattern        = "Aktivierung durch Musterübereinstimmung"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Deaktiviert"
Enable                      = "Aktiviert"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Roaming-Dynamik" 
Lowest                      = "Am niedrigsten"
MediumLow                   = "Mittel-niedrig"
Medium                      = "Mittel"
MediumHigh                  = "Mittel-hoch"
Highest                     = "Am höchsten"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Spanish
;*******************************************************************************************
[Strings.0c0a]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "Radio Encendido/Apagado"
CountryRegion24G            = "Región País (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Región País (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Ambiente de Multimedia/Juego"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Banda preferida"
NoPref                      = "Sin preferencias"
Band_24G                    = "Preferir la banda de 2,4 GHz"
Band_5G                     = "Preferencia de banda 5 GHz"
Band_6G                     = "Preferencia de banda 6 GHz"
DisableWakeOnMagic          = "Magic Packet de reactivación"
DisableWakeOnPattern        = "Coincidencia de patrones de reactivación"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Desactivado"
Enable                      = "Activado"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Agresividad de itinerancia" 
Lowest                      = "Mínimo"
MediumLow                   = "Bajo"
Medium                      = "Mediano"
MediumHigh                  = "Alto"
Highest                     = "Máximo"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Brazilian Portuguese
;*******************************************************************************************
[Strings.0416]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "Rádio Ligado/Desligado"
CountryRegion24G            = "País Região (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "País Região (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Ambiente de Multimedia/Jogo"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Banda preferencial"
NoPref                      = "Sem preferência"
Band_24G                    = "Preferir banda de 2,4 GHz"
Band_5G                     = "Preferir banda de 5 GHz"
Band_6G                     = "Preferir banda de 6 GHz"
DisableWakeOnMagic          = "Pacote Mágico do Wake on"
DisableWakeOnPattern        = "Correspondência de padrão do Wake on"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Desabilitado"
Enable                      = "Habilitado"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Agressividade de roaming" 
Lowest                      = "Mais baixo"
MediumLow                   = "Média a baixa"
Medium                      = "Média"
MediumHigh                  = "Média a alta"
Highest                     = "Mais alto"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Dutch
;*******************************************************************************************
[Strings.0413]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "Radio Aan/Uit"
CountryRegion24G            = "Land regio (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Land regio (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Multimedia/Spelomgeving"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Voorkeursband"
NoPref                      = "Geen voorkeur"
Band_24G                    = "Voorkeur voor 2,4-GHz band"
Band_5G                     = "5 GHz band"
Band_6G                     = "6 GHz band"
DisableWakeOnMagic          = "Activeren na Magic-pakket"
DisableWakeOnPattern        = "patroonovereenkomst"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Uitgeschakeld"
Enable                      = "Ingeschakeld"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Inc."
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Agressiviteit bij roamen" 
Lowest                      = "Laagste"
MediumLow                   = "Laag"
Medium                      = "Normaal"
MediumHigh                  = "Hoog"
Highest                     = "Hoogste"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Russian
;*******************************************************************************************
[Strings.0419]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "Радио Вкл/Выкл"
CountryRegion24G            = "трана/регион (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Страна/регион (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Мультимедийная/Игровая среда"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Предпочитаемая частота"
NoPref                      = "Нет предпочтений"
Band_24G                    = "Предпочитать частоту 2,4 ГГц"
Band_5G                     = "диапазон 5 ГГц предпочтительней."
Band_6G                     = "диапазон 6 ГГц предпочтительней."
DisableWakeOnMagic          = "Пробуждение пакетом Magic Packet"
DisableWakeOnPattern        = "Пробуждение при соответствии шаблону"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "Transmit Power Level"
UAPSDSupport                = "U-APSD Support"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Выключено"
Enable                      = "Включено"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Агрессивность роуминга" 
Lowest                      = "Мин."
MediumLow                   = "Средн.-мин."
Medium                      = "Средн."
MediumHigh                  = "Средн.-макс."
Highest                     = "Макс."

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"

;*******************************************************************************************
; Strings --- Ukrainian
;*******************************************************************************************
[strings.0422]
Provider                    = "MediaTek"
MediaTek                    = "MediaTek, Inc."

Generic.DeviceDesc          = "MediaTek 802.11AC Wireless LAN Card"
Generic.DeviceDescEx        = "MediaTek Wi-Fi 6/6E Wireless LAN Card"
MT7921.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7921 Wireless LAN Card"
MT7921.DeviceDescExB        = "MediaTek Wi-Fi 6 MT7921"
MT7921.DeviceDescExC        = "MediaTek MT7921 Wi-Fi 6 802.11ax PCIe Adapter"
RZ608.DeviceDescExA         = "RZ608 Wi-Fi 6E 80MHz"
RZ616.DeviceDescExA         = "RZ616 Wi-Fi 6E 160MHz"
MT7922.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7922 160MHz Wireless LAN Card"
MT7922.DeviceDescExB        = "MediaTek Wi-Fi 6E MT7922 160MHz"
RZ616.DeviceDescExC         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz PCIe Adapter"
RZ616.DeviceDescExD         = "MediaTek Wi-Fi 6E MT7922 (RZ616) 160MHz Wireless LAN Card"
MT7920.DeviceDescExA        = "MediaTek Wi-Fi 6 MT7920 Wireless LAN Card"
MT7902.DeviceDescExA        = "MediaTek Wi-Fi 6E MT7902 Wireless LAN Card"
MT7902.DeviceDescExB        = "MediaTek Wi-Fi MT7902 Wireless LAN Card"
MT7902.DeviceDescExC        = "MediaTek Wi-Fi 6 MT7902LEN Wireless LAN Card"
INSTALL_DISK_STR            = "Wireless 11AC PCI Installation Disk"

Generic.Service.DispName    = "Mediatek PCI LE Extensible Wireless LAN Card Driver"
ServiceName                 = "mtkwlex"

;
; Parameters
;
RadioOnOff                  = "бездротовий пристрій ВІДЧИНЕНО/закрити"
CountryRegion24G            = "Країна Регіон (2.4GHz)"
CountryRegion24G_0          = "#0 (1 - 11)"
CountryRegion24G_1          = "#1 (1 - 13)"
CountryRegion24G_2          = "#2 (10 - 11)"
CountryRegion24G_3          = "#3 (10 - 13)"
CountryRegion24G_4          = "#4 (14)"
CountryRegion24G_5          = "#5 (1 - 14)"
CountryRegion24G_6          = "#6 (3 - 9)"
CountryRegion24G_7          = "#7 (5 - 13)"
CountryRegion5G             = "Країна Регіон (5GHz)"
CountryRegion5G_0           = "#0 (36 - 64,149 - 165)"
CountryRegion5G_1           = "#1 (36 - 140)"
CountryRegion5G_2           = "#2 (36 - 64)"
CountryRegion5G_3           = "#3 (52 - 64,149 - 161)"
CountryRegion5G_4           = "#4 (149 - 165)"
CountryRegion5G_5           = "#5 (149 - 161)"
CountryRegion5G_6           = "#6 (36 - 48)"
CountryRegion5G_7           = "#7 (36 - 165)"
CountryRegion5G_8           = "#8 (52 - 64)"
CountryRegion5G_9           = "#9 (36 - 116,132 - 165)"
CountryRegion5G_10          = "#10 (36 - 48,149 - 165)"
CountryRegion5G_11          = "#11 (36 - 120,149 - 161)"
CountryRegion5G_12          = "#12 (36 - 140)"
CountryRegion5G_13          = "#13 (52 - 161)"
CountryRegion5G_14          = "#14 (36 - 116,136 - 165)"
CountryRegion5G_15          = "#15 (149 - 173)"
CountryRegion5G_16          = "#16 (36 - 173)"
CountryRegion5G_17          = "#17 (36 - 64,132 - 140)"
IEEE802_11h                 = "IEEE802.11h"
SmartScan                   = "Мультимедійне/ігрове середовище"
CurrPhyMode                 = "802.11ax/ac/n/abg"
Phy_11ax                    = "802.11ax"
Phy_11ac                    = "802.11ac"
Phy_11n                     = "802.11n"
Phy_11abg                   = "802.11a/b/g"
BWSelection24G              = "2.4GHz channel bandwidth"
BWSelection5G               = "5GHz channel bandwidth"
BWSelection6G               = "6GHz channel bandwidth"
BW_Auto                     = "Auto"
BW_20                       = "20MHz only"
BandSelection               = "Band Selection"
Band_All                   = "All Band"
Band24G                     = "2.4G Only"
Band5G                      = "5G Only"
Band6G                      = "6G Only"
PreferredBand               = "Бажаний діапазон"
NoPref                      = "Без переваг"
Band_24G                    = "Віддаю перевагу діапазону 2.4GHz"
Band_5G                     = "Віддаю перевагу 5GHz діапазону"
Band_6G                     = "Віддаю перевагу 6GHz діапазону"
DisableWakeOnMagic          = "Пробудження по Magic пакет"
DisableWakeOnPattern        = "пробудження за шаблоном"
DisableARPOffload           = "ARP Offload for WOWLAN"
DisableGTKRekey             = "GTK Rekey for WOWLAN"
TxPowerLevel                = "передавати рівень потужності"
UAPSDSupport                = "U-APSD підтримка"
AMSDUTx                     = "AMSDU Tx"
AMSDURx                     = "AMSDU Rx"
Disable                     = "Вимкнено"
Enable                      = "Увімкнено"
BaldEagle_SSID              = "amz?;'seimdf^&j$#@ksjdo*(hq!"

CHANNEL                     = "1"
WPS_DEVNAME_DEF_STR         = "MediaTek Client"
WPS_DEVNAME_CUSTOMER1       = "Corega Client"

WirelessMode                = "Wireless Mode"
WirelessModeBoth            = "Both"
WirelessMode24G             = "2.4G"
WirelessMode5G              = "5G"
WirelessModeAuto            = "Auto"

RoamingAggressiveness       = "Агресивність роумінгу" 
Lowest                      = "Найнижчий"
MediumLow                   = "Середній-Низький"
Medium                      = "Середній"
MediumHigh                  = "Середньо-високий"
Highest                     = "Найвищий"

BACKGROUNDSCAN              = "Background Scan"
ALLOW                       = "Allow"
DISALLOW                    = "Disallow"

PMF                         = "Protect Management Frame"
CHANNEL_MODE                = "Channel Mode"
ChannelMode_0               = "2.4G"
ChannelMode_1               = "2.4G + 5G"
ChannelMode_2               = "5G Only"

PreferABand                 = "Prefer 5G"
LowpowerStr                 = "Power Saving"
